**Mosfet Selection**

It is known that switching element must be withstand the maximum input voltage and the secondary voltage reflected value. On the other hand, spikes which are caused by leakage inductances should be considered. MOSFET VDS can be calculated from below formula:

Where;

*estimated to be thirty percent of the*

1.3 additional safety factor